**3 Introduction and Motivations**

**3.1 Background**

In an electrical grid system, power generation and consumption should be balanced at all times because an imbalance between them may lead to problems including voltage fluctuation and even power outage. Therefore, a grid system is designed to accommodate the maximum peak load, which occurs no more than a few times a year.[1] The costs of meeting the peak demand have been significant as generators, transmission lines, circuit breakers, and transformers have been largely underutilized during off-peak hours.[2] The daily peak demand usually occurs around 5:30 PM, due to office use, domestic demand, and, in certain seasons, the fall darkness.[3]

Our study first started with a conjecture that, along with the already existing factors mentioned above, the simultaneous charging of electric vehicles(EVs) during evening hours would further raise the daily peak load. Although EVs only comprise a small portion of the automotive market at the moment, the sales of EVs have surpassed a million since their mass market began only five years ago.[4] Thus, we supposed that, in near future, our grid system will have to be able to supply enough power required to charge hundreds of thousands of EVs at the same time and that it would be a meaningful work to propose a model that analyzes and resolves this issue.

A smart microgrid, a modern and localized network, has been considered one possible solution because of its active decentralized management of demand. Unlike a traditional, centralized grid (macrogrid), a microgrid actively responds to locally collected demand information. Therefore, in this study, we have modeled a smart microgrid with EVs, which collects local power consumption information and determines when each of its member EVs should be charged.

**3.1 Objectives**

This study uses a mathematical model and simulation to analyze the power consumption of EVs in a microgrid when different charging plans are applied. Our study addresses the following questions:

* How does the total power consumption of the microgrid change throughout a day?
* When does the peak demand occur?
* How and how much can this peak demand be alleviated?
* How does the smart microgrid find its optimal solution?
* How does the effect of this solution change as some of the independent variables of the model vary?

[1] Alt, Lowell (2006). [*Energy Utility Rate Setting*](http://books.google.com.au/books?id=RW3tycY4TToC). Lulu.com. p. 66. [ISBN](https://en.wikipedia.org/wiki/International_Standard_Book_Number) [1411689593](https://en.wikipedia.org/wiki/Special:BookSources/1411689593). Retrieved 25 June 2013.

[2] Peterson et al., The economics of using plug-in hybrid electric vehicle battery packs for grid storage, Journal of Power Sources, 2010.

[3] Landsberg, Dennis R.; Ronald Stewart (1980). [Improving Energy Efficiency in Buildings: A Management Guide](http://books.google.com.au/books?id=M0EnqtFxW3cC). SUNY Press. p. 456. [ISBN](https://en.wikipedia.org/wiki/International_Standard_Book_Number) [1438409990](https://en.wikipedia.org/wiki/Special:BookSources/1438409990).

[4] Jeff Cobb (2015-09-16). ["One Million Global Plug-In Sales Milestone Reached"](http://www.hybridcars.com/one-million-global-plug-in-sales-milestone-reached/). HybridCars.com. Retrieved 2015-09-16. U.S. cumulative sales since 2008 totaled 363,265 highway legal plug-in electric passenger cars through August 2015.